|  |  |
| --- | --- |
|  | Checklist 04-3: **Pouring Foundation Walls (TS3)** |
| MC Development Corp. | Project: | Contractor: |
| **Number** | **Checkpoints** | BI | DI | AI |
| **1** | Status of previous TS inspections are approved by the PM/DNV |  |  |  |
| **Comment** |  |
| **2** | Forms in correct location, completed, plumb, properly supported |  |  |  |
| **Comment** |  |
| **3** | Proper concrete mix design is ordered (per exposure conditions, spec, and code) |  |  |  |
| **Comment** |  |
| **4** | Electrical conduit installed if required |  |  |  |
| **Comment** |  |
| **5** | Proper vibrator in place and used correctly to consolidate concrete |  |  |  |
| **Comment** |  |
| **6** | Adequate form release agent has been applied to the formwork |  |  |  |
| **Comment** |  |
| **7** | Top of concrete levelled off, trowelled to required finish, and cleaned of excess concrete? |  |  |  |
| **Comment** |  |
| **8** | The finished concrete covered properly (curing) |  |  |  |
| **Comment** |  |
| **9** | Finished surface is smooth and in a good condition |  |  |  |
| **Comment** |  |
| **Quality Scores and Completion Sign-off** |
| **Inspection#**Quality 5 4 3 2 1 Notes:On-Time 5 4 3 2 1 Notes:Sign and date\*: Cell # / ID #: Signed: Date: Task has been verified complete and in compliance with contract drawings and specifications except for non-conformances and incomplete items reported above. |
| **BI=** Inspection **B**efore task begin **-----------DI=** Inspection **D**uring task in-process --------**AI=** Inspection **A**fter task completed*Quality Score**5 = 100% NO problems 4 = 1 minor problems 3 = Hotspot or 2-3 minor 2 = 6+ or major problems 1 = Excessive problems****On-Time Score*** *5 = On Time 4 = Late 3 = Late by 1 day 2 = Late by 2 days 1 = Late more than 2 days****Safety Score*** *5 = 100% NO problems 4 = 1 minor problem 3 = Hotspot or 2-3 minor 2= 4+ or major problem 1= Injury* |