|  |  |
| --- | --- |
|  | Checklist 10-3: **Drill the Framing (TS3)** |
| MC Development Corp. | Project: | Contractor: |
| **Number** | **Checkpoints** | BI | DI | AI |
| **1** | Double check; Layout is complete and all required boxes are Nailed up according to the script markings on the walls and floor |  |  |  |
| **Comment** |  |
| **2** | Safety first when drilling; safety glasses |  |  |  |
| **Comment** |  |
| **3** | Plumbing pipes are marked, and No damaging to plumbing pipes |  |  |  |
| **Comment** |  |
| **4** | Proper drill has been chosen |  |  |  |
| **Comment** |  |
| **5** | holes within 8 inches above or below a line of boxes |  |  |  |
| **Comment** |  |
| **6** | holes within the back-splash area of the kitchen counter |  |  |  |
| **Comment** |  |
| **7** | Sizes, height, and locations of the holes are correct |  |  |  |
| **Comment** |  |
| **8** | the holes straight aligned and at the same height.  |  |  |  |
| **Comment** |  |
| **9** | a nail plate is nailed on the stud if the hole is too close to the nailing surface |  |  |  |
| **Comment** |  |
| **Quality Scores and Completion Sign-off** |
| **Inspection#**Quality 5 4 3 2 1 Notes:On-Time 5 4 3 2 1 Notes:Sign and date\*: Cell # / ID #: Signed: Date: Task has been verified complete and in compliance with contract drawings and specifications except for non-conformances and incomplete items reported above. |
| **BI=** Inspection **B**efore task begin **-----------DI=** Inspection **D**uring task in-process --------**AI=** Inspection **A**fter task completed*Quality Score**5 = 100% NO problems 4 = 1 minor problems 3 = Hotspot or 2-3 minor 2 = 6+ or major problems 1 = Excessive problems****On-Time Score*** *5 = On Time 4 = Late 3 = Late by 1 day 2 = Late by 2 days 1 = Late more than 2 days****Safety Score*** *5 = 100% NO problems 4 = 1 minor problem 3 = Hotspot or 2-3 minor 2= 4+ or major problem 1= Injury* |